-- BEGIN LanSafe III MIB Defs
--      @(#)smi.defs	6.2 8/21/93 - STREAMware TCP/IP  source
--
-- Copyrighted as an unpublished work.
-- (c) Copyright 1987-1993 Lachman Technology, Inc.
-- All rights reserved.
--
--      SCCS IDENTIFICATION

-- This is the smi.defs file that needs to be concatenated with the
-- <smux_peer>.defs file

internet             iso.3.6.1
directory            internet.1
mgmt                 internet.2
experimental         internet.3
private              internet.4
enterprises          private.1

mib-2		mgmt.1

-- automatically generated by mosy 8.0 #1  Tue Dec 1 15:14:16 CST 1992, do not edit!

-- object definitions compiled from UPS-MIB

upsMIB               mib-2.33
upsObjects           upsMIB.1
csi                  enterprises.1039
products             csi.1
csimgmt              csi.2
mconfig              csimgmt.1
upsIdent             upsObjects.1
upsBattery           upsObjects.2
upsInput             upsObjects.3
upsOutput            upsObjects.4
upsBypass            upsObjects.5
upsAlarm             upsObjects.6
upsTest              upsObjects.7
upsControl           upsObjects.8
upsConfig            upsObjects.9

mconfigNumTrapReceivers mconfig.1        INTEGER         read-only       mandatory
mconfigTrapReceiverTable mconfig.2        Aggregate       not-accessible  mandatory
mconfigTrapReceiverEntry mconfigTrapReceiverTable.1 Aggregate       not-accessible  mandatory
trapIndex            mconfigTrapReceiverEntry.1 INTEGER         read-only       mandatory
receiverAddr         mconfigTrapReceiverEntry.2 IpAddress       read-write      mandatory
communityString      mconfigTrapReceiverEntry.3 DisplayString   read-write      mandatory
severity             mconfigTrapReceiverEntry.4 INTEGER         read-write      mandatory
acceptThisReceiver   mconfigTrapReceiverEntry.5 INTEGER         read-write      mandatory
upsIdentManufacturer upsIdent.1       DisplayString   read-only       mandatory
upsIdentModel        upsIdent.2       DisplayString   read-only       mandatory
upsIdentUPSSoftwareVersion upsIdent.3       DisplayString   read-only       mandatory
upsIdentAgentSoftwareVersion upsIdent.4       DisplayString   read-only       mandatory
upsIdentName         upsIdent.5       DisplayString   read-write      mandatory
upsIdentAttachedDevices upsIdent.6       DisplayString   read-write      mandatory
upsBatteryStatus     upsBattery.1     INTEGER         read-only       mandatory
upsSecondsOnBattery  upsBattery.2     INTEGER         read-only       mandatory
upsEstimatedMinutesRemaining upsBattery.3     INTEGER         read-only       mandatory
upsEstimatedChargeRemaining upsBattery.4     INTEGER         read-only       mandatory
upsBatteryVoltage    upsBattery.5     INTEGER         read-only       mandatory
upsBatteryCurrent    upsBattery.6     INTEGER         read-only       mandatory
upsBatteryTemperature upsBattery.7     INTEGER         read-only       mandatory
upsInputLineBads     upsInput.1       INTEGER         read-only       mandatory
upsInputNumLines     upsInput.2       INTEGER         read-only       mandatory
upsInputTable        upsInput.3       Aggregate       not-accessible  mandatory
upsInputEntry        upsInputTable.1  Aggregate       not-accessible  mandatory
upsInputLineIndex    upsInputEntry.1  INTEGER         not-accessible  mandatory
upsInputFrequency    upsInputEntry.2  INTEGER         read-only       mandatory
upsInputVoltage      upsInputEntry.3  INTEGER         read-only       mandatory
upsInputCurrent      upsInputEntry.4  INTEGER         read-only       mandatory
upsInputTruePower    upsInputEntry.5  INTEGER         read-only       mandatory
upsOutputSource      upsOutput.1      INTEGER         read-only       mandatory
upsOutputFrequency   upsOutput.2      INTEGER         read-only       mandatory
upsOutputNumLines    upsOutput.3      INTEGER         read-only       mandatory
upsOutputTable       upsOutput.4      Aggregate       not-accessible  mandatory
upsOutputEntry       upsOutputTable.1 Aggregate       not-accessible  mandatory
upsOutputLineIndex   upsOutputEntry.1 INTEGER         not-accessible  mandatory
upsOutputVoltage     upsOutputEntry.2 INTEGER         read-only       mandatory
upsOutputCurrent     upsOutputEntry.3 INTEGER         read-only       mandatory
upsOutputPower       upsOutputEntry.4 INTEGER         read-only       mandatory
upsOutputPercentLoad upsOutputEntry.5 INTEGER         read-only       mandatory
upsBypassFrequency   upsBypass.1      INTEGER         read-only       mandatory
upsBypassNumLines    upsBypass.2      INTEGER         read-only       mandatory
upsBypassTable       upsBypass.3      Aggregate       not-accessible  mandatory
upsBypassEntry       upsBypassTable.1 Aggregate       not-accessible  mandatory
upsBypassLineIndex   upsBypassEntry.1 INTEGER         not-accessible  mandatory
upsBypassVoltage     upsBypassEntry.2 INTEGER         read-only       mandatory
upsBypassCurrent     upsBypassEntry.3 INTEGER         read-only       mandatory
upsBypassPower       upsBypassEntry.4 INTEGER         read-only       mandatory
upsAlarmsPresent     upsAlarm.1       INTEGER         read-only       mandatory
upsAlarmTable        upsAlarm.2       Aggregate       not-accessible  mandatory
upsAlarmEntry        upsAlarmTable.1  Aggregate       not-accessible  mandatory
upsAlarmId           upsAlarmEntry.1  INTEGER         not-accessible  mandatory
upsAlarmDescr        upsAlarmEntry.2  INTEGER         read-only       mandatory
upsAlarmTime         upsAlarmEntry.3  INTEGER         read-only       mandatory
upsTestId            upsTest.1        INTEGER         read-write      mandatory
upsTestSpinLock      upsTest.2        INTEGER         read-write      mandatory
upsTestResultsSummary upsTest.3        INTEGER         read-only       mandatory
upsTestResultsDetail upsTest.4        DisplayString   read-only       mandatory
upsTestStartTime     upsTest.5        INTEGER         read-only       mandatory
upsTestElapsedTime   upsTest.6        INTEGER         read-only       mandatory
upsShutdownType      upsControl.1     INTEGER         read-write      mandatory
upsShutdownAfterDelay upsControl.2     INTEGER         read-write      mandatory
upsStartupAfterDelay upsControl.3     INTEGER         read-write      mandatory
upsRebootWithDuration upsControl.4     INTEGER         read-write      mandatory
upsAutoRestart       upsControl.5     INTEGER         read-write      mandatory
upsConfigInputVoltage upsConfig.1      INTEGER         read-write      mandatory
upsConfigInputFreq   upsConfig.2      INTEGER         read-write      mandatory
upsConfigOutputVoltage upsConfig.3      INTEGER         read-write      mandatory
upsConfigOutputFreq  upsConfig.4      INTEGER         read-write      mandatory
upsConfigOutputVA    upsConfig.5      INTEGER         read-only       mandatory
upsConfigOutputPower upsConfig.6      INTEGER         read-only       mandatory
upsConfigLowBattTime upsConfig.7      INTEGER         read-write      mandatory
upsConfigAudibleStatus upsConfig.8      INTEGER         read-write      mandatory
upsConfigLowVoltageTransferPoint upsConfig.9      INTEGER         read-write      mandatory
upsConfigHighVoltageTransferPoint upsConfig.10     INTEGER         read-write      mandatory


-- END LanSafe III MIB Defs
